Disasm.asm documentation:

**Functions:**

[address\_to\_hex 2](#_Toc151830241)

# address\_to\_hex

Take address and change it to human readable format. Furthermore, write the results to line variable.

Used functions by this function:

* convert\_half\_byte\_to\_HEX